{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["相机"],"not_rendered":{"charts":0,"images":15,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"相机","index":0,"n_rows":15,"n_cols":12,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,11],[2,1,14,1],[2,4,14,4],[2,2,14,2],[2,3,7,3],[2,5,3,5],[2,6,3,6],[7,5,8,5],[7,6,8,6],[8,3,14,3]]}
["深时相机检验记录明细"]
["序号","工厂\n确认日期","产品名称","相机颜色","检测数量","不良台数","不良率","不良现象","图片","原因分析","对策","备注"]
[1,"2023.7.4","深时相机","红色",13,2,{"$f":"F3/E3","v":0.15384615384615385},"雷达表面有伤痕",null,null,null,"本次可接收\n下次生产时要改善"]
[2,{"$nulls":6},"雷达表面有伤痕",null,null,null,"不接收，需要更换"]
[3,{"$nulls":4},1,{"$f":"F5/E3","v":7.6923076923076927E-2},"前盖伤痕",null,null,null,"不接收，需要更换"]
[4,{"$nulls":4},1,{"$f":"F6/E3","v":7.6923076923076927E-2},"显示屏有水纹",null,null,null,"不接收，需要更换"]
[5,{"$nulls":4},2,{"$f":"F7/E3","v":0.15384615384615385},"显示屏伤痕",null,null,null,"本次可接收\n下次生产时要改善"]
[6,{"$nulls":4},2,{"$f":"F8/13","v":0.15384615384615385},"提手胶垫伤痕",null,null,null,"本次可接收\n下次生产时要改善"]
[9,null,null,"蓝色",null,null,null,"提手胶垫伤痕",null,null,null,"不接收，需要更换"]
[7,{"$nulls":4},1,{"$f":"F10/E3","v":7.6923076923076927E-2},"提手胶垫贴付不均匀",null,null,null,"本次可接收\n下次生产时要改善"]
[8,{"$nulls":4},"全数",1,"电池盒内灰尘多",null,null,null,"吹拭干净，接收\n下次生产时要改善"]
[10,{"$nulls":4},2,{"$f":"F12/E3","v":0.15384615384615385},"显示屏伤痕",null,null,null,"本次可接收\n下次生产时要改善"]
[11,{"$nulls":4},1,{"$f":"F13/E3","v":7.6923076923076927E-2},"有胶残留，有堵孔的隐患",null,null,null,"擦拭干净，接收\n下次生产时要改善"]
[12,{"$nulls":4},2,{"$f":"F14/E3","v":0.15384615384615385},"提手有胶残留",null,null,null,"擦拭干净，接收\n下次生产时要改善"]
[13,{"$nulls":4},1,{"$f":"F15/E3","v":7.6923076923076927E-2},"有胶残留",null,null,null,"擦拭干净，接收\n下次生产时要改善"]